{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["投标总价","四川省南充市保安服务有限公司6楼办公室装修改造工程量清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"投标总价","index":0,"n_rows":12,"n_cols":3,"rows_kept":12,"merged":[[0,0,0,2],[4,0,5,0],[4,1,5,1],[4,2,5,2],[6,0,6,2],[12,0,12,2]],"flags":["formulas_cached_only"]}
["投 标 总 价"]
["\r\n招　　标　　人:","四川省南充市保安服务有限公司",""]
["工  程　名  称:","四川省南充市保安服务有限公司6楼办公室装修改造",""]
["投标总价(小写):",null,""]
["(大写):",null,""]
[]
[""]
["投　标　人:"," ",""]
["",null,""]
["　　　法定代表人 \r\n或其授权人:"," ",""]
["       ","(签字或盖章)",""]
["  时      间:"," ",""]

{"sheet":"四川省南充市保安服务有限公司6楼办公室装修改造工程量清单","index":1,"n_rows":44,"n_cols":8,"rows_kept":44,"merged":[[0,0,0,7],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,1,6],[1,7,3,7],[2,5,3,5],[2,6,3,6],[4,1,4,2],[11,1,11,2],[12,1,12,2],[23,1,23,2],[24,1,24,2],[27,1,27,2],[28,1,28,2],[34,1,34,2],[35,1,35,2],[37,1,37,2],[38,1,38,2],[42,1,42,2],[43,0,43,5]],"flags":["formulas_cached_only"]}
["四川省南充市保安服务有限公司6楼办公室装修改造工程量清单"]
["序号","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","备注"]
["","","","","","全费用综合单价","合价"]
["","","","","","",""]
[" ","拆除工程 ",""," "," "," "," "]
["1","原墙壁墙布铲除","1.铲除部位名称 ：墙面\r\n2.铲除部位的截面尺寸：详设计","m2","178.84"]
["2","木作墙裙拆除","1.名称：木作墙裙拆除\r\n2.其它;详设计","m2","107.35"]
["3","木地板拆除","1.拆除的基层类型 ：详设计\r\n2.龙骨及饰面种类：详设计","m2","23.1"]
["4","地面水泥层拆除","1. 拆除部位 ：地面\r\n2. 抹灰层种类：水泥砂浆","m2","47.13"]
["5","地毯拆除","1.名称：地毯拆除\r\n2.其它;详设计","m2","47.17"]
["6","拆除后墙地面局部修复","1.名称：拆除后墙地面局部修复","m2","382.24"]
[" ","分部小计 ",""," "," "]
[" ","装饰工程 ",""," "," "]
["7","800*800玻化砖","1.找平层材料种类、厚度：1:3水泥砂浆20mm厚\r\n2.结合层厚度、砂浆配合比：20mm厚1:3干硬性水泥砂浆，上洒1-2厚干水泥并洒适量清水\r\n3.面层材料品种、规格：800*800玻化砖\r\n4.嵌缝材料种类：综合","m2","76.21"]
["8","15mm天然黑金花石材","1.找平层材料种类、厚度：1:3水泥砂浆20mm厚\r\n2.结合层厚度、砂浆配合比：20mm厚1:3干硬性水泥砂浆，上洒1-2厚干水泥并洒适量清水\r\n3.面层材料品种、规格：门槛石 15mm天然黑金花石材\r\n4.嵌缝材料种类：综合","m2","1.11"]
["9","脲醛美缝剂美缝","脲醛美缝剂美缝","m2","76.21"]
["10","内墙面乳胶漆（含腻子）","1.基层类型：综合\r\n2.腻子种类：成品腻子\r\n3.刮腻子要求：清理基层，修补，砂纸打磨；满刮腻子\r\n4.油漆品种、刷漆遍数：乳胶漆底漆一遍面漆两遍","m2","306.03"]
["11","天棚面乳胶漆（含腻子）","1.基层类型：综合\r\n2.腻子种类：成品腻子\r\n3.刮腻子要求：清理基层，修补，砂纸打磨；满刮腻子\r\n4.油漆品种、刷漆遍数：乳胶漆底漆一遍面漆两遍","m2","88.92"]
["12","304-10目室内精钢防护网","1.名称：304-10目室内精钢防护网\r\n2.其它：详设计","m2","9.2"]
["13","8mm304实心不锈钢防护栏","1.名称：8mm304实心不锈钢防护栏\r\n2.其它：详设计","m2","12"]
["14","双音质防盗门","1.门类型：钢质防盗门\r\n2.五金材料：铰链、拉手、门锁、闭门器、门扎头、闭门器、指纹锁等特殊五金均包含在综合单价中\r\n3.洞周围紧固件、密封材料、发泡剂、埋件、连接件、简易脚手架等相关费用综合在单价中\r\n4.油漆、防火漆、颜色、样式等满足业主要求综合在单价中\r\n5.其他做法满足设计及相关规范要求","m2","3.78"]
["15","B级指纹锁","1.锁品种:B级指纹锁\r\n2.锁规格:详设计","套","2"]
["16","瓷砖踢脚线（800*800地砖现切）","1.粘结层厚度、材料种类：水泥浆粘贴\r\n2.面层材料品种、规格：800*800地砖现切","m2","2.81"]
[" ","分部小计 ",""," "," "]
[" ","其他工程 ",""," "," "]
["17","金属百叶窗","1.名称：金属百叶窗\r\n2.其它：详设计","m2","62"]
["18","建渣外运（运距5km)","1.余方品种：场地内土方、石方、建渣等\r\n2.外运运距：5km\r\n3.外运处置费用（或倒场费）由投标人自行考虑在单价内\r\n4.其它做法满足技术及相关规范要求","m3","15"]
[" ","分部小计 ",""," "," "]
[" ","安装工程 ",""," "," "]
["19","带保护接点暗装插座","1.名称：带保护接点暗装插座\r\n2.型号、规格：10A，250V \r\n3.安装方式：暗装\r\n4.其他：满足设计、规范及相关技术要求","个","12"]
["20","筒灯","1.名称：筒灯\r\n2.型号、规格：综合\r\n3.安装方式：吸顶安装\r\n4.其他详设计及满足规范要求","套","18"]
["21","600*600吸顶灯 48W","1.名称：600*600吸顶灯 48W\r\n2.型号、规格：综合\r\n3.安装方式：吸顶安装\r\n4.其他详设计及满足规范要求","套","6"]
["22","新装门禁","1.名称 :新装门禁\r\n2.其它：详设计","套","1"]
["23","配线 BV-1.5mm2","1.配线形式：管内穿线\r\n2.导线型号、材质、规格： BV-1.5mm2\r\n3.敷设部位或线制：照明线路","m","15"]
[" ","分部小计 ",""," "," "]
[" ","专业措施项目 ",""," "," "," "," "]
[24,"脚手架搭拆"," ","项","1"]
[" ","分部小计 ",""," "," "]
[" ","暂估价项目",null," "," "," "," "]
[25,"办公桌","详设计及满足规范要求","套",12]
[26,"办公椅","详设计及满足规范要求","把",12]
[27,"文件柜","详设计及满足规范要求","组",6]
[" ","分部小计 ",null," "," "]
["合    计","","","","",""]